(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 353)
    (zones 0)
    (modules 45)
    (nets 58)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.2)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8 1.8)
    (pad_drill 1)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 42.206 92.824)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x01008_7ffffffe)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad3)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 GND)
  (net 4 "Net-(D2-Pad2)")
  (net 5 +5V)
  (net 6 -9V)
  (net 7 /RESET)
  (net 8 +9V)
  (net 9 "Net-(U1-Pad6)")
  (net 10 +3V3)
  (net 11 "Net-(J2-Pad1)")
  (net 12 "Net-(D5-Pad1)")
  (net 13 "Net-(U4-Pad6)")
  (net 14 "Net-(C7-Pad2)")
  (net 15 "Net-(C7-Pad1)")
  (net 16 "Net-(C8-Pad2)")
  (net 17 "Net-(C8-Pad1)")
  (net 18 "Net-(D2-Pad1)")
  (net 19 "Net-(D3-Pad2)")
  (net 20 "Net-(D4-Pad1)")
  (net 21 "Net-(J2-Pad6)")
  (net 22 "Net-(J2-Pad5)")
  (net 23 "Net-(J2-Pad4)")
  (net 24 "Net-(J2-Pad3)")
  (net 25 "Net-(J2-Pad2)")
  (net 26 "Net-(R5-Pad2)")
  (net 27 "Net-(U4-Pad32)")
  (net 28 "Net-(U4-Pad1)")
  (net 29 "Net-(U4-Pad2)")
  (net 30 "Net-(U4-Pad30)")
  (net 31 "Net-(U4-Pad3)")
  (net 32 "Net-(U4-Pad29)")
  (net 33 "Net-(U4-Pad28)")
  (net 34 "Net-(U4-Pad5)")
  (net 35 "Net-(U4-Pad27)")
  (net 36 "Net-(U4-Pad26)")
  (net 37 "Net-(U4-Pad7)")
  (net 38 "Net-(U4-Pad25)")
  (net 39 "Net-(U4-Pad24)")
  (net 40 "Net-(U4-Pad11)")
  (net 41 "Net-(U4-Pad20)")
  (net 42 "Net-(U4-Pad19)")
  (net 43 "Net-(U4-Pad18)")
  (net 44 "Net-(U4-Pad17)")
  (net 45 "Net-(R12-Pad2)")
  (net 46 "Net-(IN1-Pad1)")
  (net 47 "Net-(LOUT1-Pad1)")
  (net 48 "Net-(MID5-Pad1)")
  (net 49 "Net-(R13-Pad1)")
  (net 50 "Net-(R12-Pad1)")
  (net 51 "Net-(RV1-Pad3)")
  (net 52 "Net-(RV2-Pad3)")
  (net 53 "Net-(RV1-Pad2)")
  (net 54 "Net-(RV2-Pad2)")
  (net 55 "Net-(GND1-Pad1)")
  (net 56 "Net-(GND2-Pad1)")
  (net 57 "Net-(U4-Pad9)")
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net +9V)
    (add_net -9V)
    (add_net /RESET)
    (add_net GND)
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(GND1-Pad1)")
    (add_net "Net-(GND2-Pad1)")
    (add_net "Net-(IN1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(LOUT1-Pad1)")
    (add_net "Net-(MID5-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(RV1-Pad2)")
    (add_net "Net-(RV1-Pad3)")
    (add_net "Net-(RV2-Pad2)")
    (add_net "Net-(RV2-Pad3)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad11)")
    (add_net "Net-(U4-Pad17)")
    (add_net "Net-(U4-Pad18)")
    (add_net "Net-(U4-Pad19)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U4-Pad20)")
    (add_net "Net-(U4-Pad24)")
    (add_net "Net-(U4-Pad25)")
    (add_net "Net-(U4-Pad26)")
    (add_net "Net-(U4-Pad27)")
    (add_net "Net-(U4-Pad28)")
    (add_net "Net-(U4-Pad29)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad30)")
    (add_net "Net-(U4-Pad32)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U4-Pad7)")
    (add_net "Net-(U4-Pad9)")
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.106 69.474 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 3.75 -0.3 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(D5-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 95.292 90.919)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference IN2 (at -0.127 -2.413) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 62.145 89.141)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference GND2 (at -0.254 2.286) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(GND2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 66.209 89.141)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference GND1 (at 0 2.25) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(GND1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5A0AB76C)
    (at 90.424 67.31)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U5 (at 3.707 -1.786) (layer F.SilkS))
    (fp_text value 74LVC1G125 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R12-Pad2)"))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R5-Pad2)"))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-6_W7.62mm placed (layer F.Cu) (tedit 5A02E8C5)
    (at 78.74 82.55 90)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 0 -3.048) (layer F.SilkS))
    (fp_text value 4N25 (at 3.81 7.41 90) (layer F.Fab))
    (fp_text user %R (at 3.81 2.54 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad3)"))
    (pad 5 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R5-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ada-base-1:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 58.42 77.47 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 47 "Net-(LOUT1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ada-base-1:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 70.228 69.85)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -4.02544 0.14732) (layer F.SilkS))
    (fp_text value 1K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 49 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 90.424 71.12)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -3.993 1.079 180) (layer F.SilkS))
    (fp_text value 220 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 45 "Net-(R12-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 50 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 86.106 69.596)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference THRU1 (at -2.35 -4.597 180) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 71.374 78.486)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at -0.12192 3.60172) (layer F.SilkS))
    (fp_text value TL072 (at 0 3.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +9V))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C8-Pad2)"))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C8-Pad1)"))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(RV2-Pad2)"))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 -9V))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(RV1-Pad2)"))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C7-Pad1)"))
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 70.358 73.152)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 3.43916 0.98552) (layer F.SilkS))
    (fp_text value "220 pF" (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 16 "Net-(C8-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 65.278 77.47 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 3.0226 0.02032 180) (layer F.SilkS))
    (fp_text value "220 pF" (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 "Net-(C7-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 15 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ada-base-1:DIP-32_995_ELL placed (layer B.Cu) (tedit 5E399DAA)
    (at 106.68 60.198 180)
    (fp_text reference U4 (at 7.874 -26.035 270) (layer B.SilkS) hide)
    (fp_text value vs1053-ada-breakout-2 (at 30.48 -12.7) (layer B.Fab))
    (pad 32 thru_hole oval (at 11.43 -2.54 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(U4-Pad32)"))
    (pad 1 thru_hole rect (at 11.43 -25.343 180) (size 1.4 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(U4-Pad1)"))
    (pad 31 thru_hole oval (at 13.97 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R5-Pad2)"))
    (pad 2 thru_hole oval (at 13.97 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U4-Pad2)"))
    (pad 30 thru_hole oval (at 16.51 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U4-Pad30)"))
    (pad 3 thru_hole oval (at 16.51 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U4-Pad3)"))
    (pad 29 thru_hole oval (at 19.05 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U4-Pad29)"))
    (pad 4 thru_hole oval (at 19.05 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /RESET))
    (pad 28 thru_hole oval (at 21.59 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U4-Pad28)"))
    (pad 5 thru_hole oval (at 21.59 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U4-Pad5)"))
    (pad 27 thru_hole oval (at 24.13 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U4-Pad27)"))
    (pad 6 thru_hole oval (at 24.13 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(U4-Pad6)"))
    (pad 26 thru_hole oval (at 26.67 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(U4-Pad26)"))
    (pad 7 thru_hole oval (at 26.67 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U4-Pad7)"))
    (pad 25 thru_hole oval (at 29.21 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(U4-Pad25)"))
    (pad 8 thru_hole oval (at 29.21 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 24 thru_hole oval (at 31.75 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U4-Pad24)"))
    (pad 9 thru_hole oval (at 31.75 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(U4-Pad9)"))
    (pad 23 thru_hole oval (at 34.29 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 +3V3))
    (pad 10 thru_hole oval (at 34.29 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 22 thru_hole oval (at 36.83 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 11 thru_hole oval (at 36.83 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(U4-Pad11)"))
    (pad 21 thru_hole oval (at 39.37 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 +3V3))
    (pad 12 thru_hole oval (at 39.37 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 20 thru_hole oval (at 41.91 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(U4-Pad20)"))
    (pad 13 thru_hole oval (at 41.91 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(GND1-Pad1)"))
    (pad 19 thru_hole oval (at 44.45 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U4-Pad19)"))
    (pad 14 thru_hole oval (at 44.45 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(GND2-Pad1)"))
    (pad 18 thru_hole oval (at 46.99 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U4-Pad18)"))
    (pad 15 thru_hole oval (at 46.99 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(RV2-Pad3)"))
    (pad 17 thru_hole oval (at 49.53 -2.597 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(U4-Pad17)"))
    (pad 16 thru_hole oval (at 49.53 -25.343 180) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(RV1-Pad3)"))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 60.706 82.042)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 3.45948 0.30988) (layer F.SilkS))
    (fp_text value 1K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 16 "Net-(C8-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 47 "Net-(LOUT1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 67.31 66.548 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -1.40716 1.81356) (layer F.SilkS))
    (fp_text value 1K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 "Net-(C7-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 49 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 61.722 77.47 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -0.10668 -1.58496 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 "Net-(C8-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 16 "Net-(C8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 61.722 66.548 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 3.556 0) (layer F.SilkS))
    (fp_text value 47K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 15 "Net-(C7-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 61.722 72.898 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 3.53568 0.46228) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 "Net-(C8-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 61.722 69.85 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 3.50012 0.61468) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 15 "Net-(C7-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 51.562 73.914)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference LOUT1 (at -4.03352 0.20828) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(LOUT1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 71.882 66.294)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference ROUT1 (at 3.69316 -1.40208) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical placed (layer F.Cu) (tedit 5C6C6C14)
    (at 51.816 77.978 270)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (fp_text reference RV2 (at 13.843 2.794) (layer F.SilkS))
    (fp_text value 10K (at 0 9.86 270) (layer F.Fab))
    (fp_text user %R (at 7.62 2.54 90) (layer F.Fab))
    (pad "" thru_hole oval (at 7.5 -2.3) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(RV2-Pad3)"))
    (pad 2 thru_hole circle (at 0 2.5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(RV2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/ALPHA-RD901F-40.step
      (offset (xyz 7.5 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm placed (layer F.Cu) (tedit 5A1DC084)
    (at 99.314 90.932 180)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference MID5 (at -0.042 2.172) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(MID5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm placed (layer F.Cu) (tedit 5A1DC084)
    (at 99.06 85.09)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference IN1 (at 0.169 2.4) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(IN1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123F placed (layer F.Cu) (tedit 587F7769)
    (at 105.156 57.912 180)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D4 (at -3.2932 -0.0124) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.905) (layer F.Fab))
    (pad 1 smd rect (at -1.4 0 180) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.4 0 180) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 -9V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123F placed (layer F.Cu) (tedit 587F7769)
    (at 105.156 72.898)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D3 (at 3.16484 -0.03556) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.905) (layer F.Fab))
    (pad 2 smd rect (at 1.4 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.4 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 +9V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_5x4.5 placed (layer F.Cu) (tedit 5BCA39CF)
    (at 105.156 63.5 270)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x4.5mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C3 (at -3.302 -3.302 180) (layer F.SilkS))
    (fp_text value CP1 (at 0 3.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.2 0 270) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 6 -9V))
    (pad 1 smd roundrect (at -2.2 0 270) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_5x4.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_5x4.5 placed (layer F.Cu) (tedit 5BCA39CF)
    (at 105.156 88.011 270)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x4.5mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C2 (at -3.569 -2.836 180) (layer F.SilkS))
    (fp_text value CP1 (at 0 3.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.2 0 270) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 3 GND))
    (pad 1 smd roundrect (at -2.2 0 270) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_5x4.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_5x4.5 placed (layer F.Cu) (tedit 5BCA39CF)
    (at 105.029 78.74 270)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x4.5mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C1 (at 3.81 -3.048 180) (layer F.SilkS))
    (fp_text value CP1 (at 0 3.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.2 0 270) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 3 GND))
    (pad 1 smd roundrect (at -2.2 0 270) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 8 +9V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_5x4.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-2 placed (layer F.Cu) (tedit 5A70A390)
    (at 112.776 86.487 270)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference U3 (at -6.477 0.254 180) (layer F.SilkS))
    (fp_text value LM78M05_TO220 (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 0.425 1.525 270) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 -1.525 270) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 -1.525 270) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 1.525 270) (size 3.05 2.75) (layers F.Paste))
    (pad 2 smd rect (at 2.1 0 270) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -4.2 2.28 270) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 1 smd rect (at -4.2 -2.28 270) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 +9V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical placed (layer B.Cu) (tedit 59FED5CC)
    (at 111.252 77.216)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference J2 (at 1.27 2.33) (layer B.SilkS))
    (fp_text value Conn_02x08_Odd_Even (at 1.27 -20.11) (layer B.Fab))
    (fp_text user %R (at 1.27 -8.89 -90) (layer B.Fab))
    (pad 16 thru_hole oval (at 2.54 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(D4-Pad1)"))
    (pad 15 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(D4-Pad1)"))
    (pad 14 thru_hole oval (at 2.54 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 13 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 12 thru_hole oval (at 2.54 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 11 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 10 thru_hole oval (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 9 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 8 thru_hole oval (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(D3-Pad2)"))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(D3-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric placed (layer F.Cu) (tedit 5B301BBD)
    (at 88.942 89.522 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at -0.254 -2.032 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 /RESET))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm placed (layer F.Cu) (tedit 5A02FE31)
    (at 82.55 71.628 180)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.048 2.032) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 /RESET))
    (pad 2 thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 /RESET))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H9.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H13mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric placed (layer F.Cu) (tedit 5B301BBE)
    (at 71.12 58.42 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -0.0166 -2.1714) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 10 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric placed (layer F.Cu) (tedit 5B301BBE)
    (at 99.781 60.249 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 3.26136 -0.01016 180) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric placed (layer F.Cu) (tedit 5B301BBE)
    (at 71.12 89.662 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -4.161 -0.087) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123F placed (layer F.Cu) (tedit 587F7769)
    (at 86.868 80.518 270)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D2 (at -3.175 -0.127 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.905 90) (layer F.Fab))
    (pad 2 smd rect (at 1.4 0 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.4 0 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric placed (layer F.Cu) (tedit 5B301BBD)
    (at 105.156 69.596)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 3.29692 -0.10668 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 48 "Net-(MID5-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric placed (layer F.Cu) (tedit 5B301BBD)
    (at 99.314 74.676)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 3.4544 0.10668) (layer F.SilkS))
    (fp_text value 10K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric placed (layer F.Cu) (tedit 5B301BBD)
    (at 90.424 74.422 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 3.81 -0.254) (layer F.SilkS))
    (fp_text value 1K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at -0.127 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 26 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric placed (layer F.Cu) (tedit 5B301BBD)
    (at 91.355 80.632 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -3.556 0 180) (layer F.SilkS))
    (fp_text value 220 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 46 "Net-(IN1-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 18 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical placed (layer F.Cu) (tedit 5C6C6C14)
    (at 51.816 58.42 270)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (fp_text reference RV1 (at 13.589 7.66064) (layer F.SilkS))
    (fp_text value 10K (at 0 9.86 270) (layer F.Fab))
    (fp_text user %R (at 7.62 2.54 90) (layer F.Fab))
    (pad "" thru_hole oval (at 7.5 -2.3) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(RV1-Pad3)"))
    (pad 2 thru_hole circle (at 0 2.5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(RV1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/ALPHA-RD901F-40.step
      (offset (xyz 7.5 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LED_THT:LED_D5.0mm_Clear placed (layer F.Cu) (tedit 5A6C9BC0)
    (at 99.822 69.723 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D5 (at 2.416 4.124) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm_Orange.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm_Clear placed (layer F.Cu) (tedit 5A6C9BC0)
    (at 99.822 79.629 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 5.52196 -3.30708) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm_Green.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 75.175 (width 0.12) (layer F.SilkS)
    (gr_text "75.175 mm" (at 79.793558 51.928507 359.9992378) (layer F.SilkS))
    (feature1 (pts (xy 117.381 56.249) (xy 117.381048 52.612586)))
    (feature2 (pts (xy 42.206 56.248) (xy 42.206048 52.611586)))
    (crossbar (pts (xy 42.206041 53.198007) (xy 117.381041 53.199007)))
    (arrow1a (pts (xy 117.381041 53.199007) (xy 116.254529 53.785413)))
    (arrow1b (pts (xy 117.381041 53.199007) (xy 116.254545 52.612571)))
    (arrow2a (pts (xy 42.206041 53.198007) (xy 43.332537 53.784443)))
    (arrow2b (pts (xy 42.206041 53.198007) (xy 43.332553 52.611601)))
  )
  (gr_text "MIDI-Lappi rev 2" (at 61.2052 58.4578) (layer B.SilkS))
  (gr_text MID5 (at 103.331 91.224) (layer B.SilkS))
  (gr_text IN2 (at 91.856 91.224) (layer B.SilkS))
  (gr_text IN1 (at 98.781 82.699) (layer B.SilkS))
  (gr_text THRU1 (at 86.021 64.884) (layer B.SilkS))
  (gr_text ROUT1 (at 75.607 64.884) (layer B.SilkS))
  (gr_text LOUT1 (at 45.531 74.049) (layer B.SilkS))
  (gr_text GND2 (at 62.018 91.427) (layer B.SilkS))
  (gr_text GND1 (at 66.209 91.427) (layer B.SilkS))
  (dimension 36.576 (width 0.12) (layer F.SilkS)
    (gr_text "36.576 mm" (at 120.819 74.536 90) (layer F.SilkS))
    (feature1 (pts (xy 117.39 56.248) (xy 120.135421 56.248)))
    (feature2 (pts (xy 117.39 92.824) (xy 120.135421 92.824)))
    (crossbar (pts (xy 119.549 92.824) (xy 119.549 56.248)))
    (arrow1a (pts (xy 119.549 56.248) (xy 120.135421 57.374504)))
    (arrow1b (pts (xy 119.549 56.248) (xy 118.962579 57.374504)))
    (arrow2a (pts (xy 119.549 92.824) (xy 120.135421 91.697496)))
    (arrow2b (pts (xy 119.549 92.824) (xy 118.962579 91.697496)))
  )
  (gr_line (start 83.862 92.824) (end 117.39 92.824) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76.242 92.824) (end 83.862 92.824) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76.115 56.248) (end 42.206 56.248) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 83.862 56.248) (end 76.115 56.248) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.39 56.248) (end 83.862 56.248) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.39 92.824) (end 117.39 56.248) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 42.206 92.824) (end 76.242 92.824) (layer Edge.Cuts) (width 0.05))
  (gr_text "RED STRIPE -9\n" (at 101.388 58.28) (layer B.SilkS))
  (gr_text "ada-base-1\nS/N -" (at 67.733 78.219) (layer B.SilkS))
  (gr_text "MIDI Lappi\nrev2" (at 60.7988 58.5848) (layer F.SilkS))
  (gr_line (start 42.206 56.248) (end 42.206 92.824) (layer Edge.Cuts) (width 0.05))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43.140754 56.515) (xy 43.140754 91.44) (xy 116.292754 91.44) (xy 116.546754 56.515)
      )
    )
  )
)
