(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 1364)
    (zones 0)
    (modules 87)
    (nets 151)
  )
  (page A)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(S1-PadB1)")
  (net 2 "Net-(S1-PadD1)")
  (net 3 "Net-(S1-PadMH1)")
  (net 4 "Net-(S1-PadMH2)")
  (net 5 "Net-(S1-PadMH3)")
  (net 6 "Net-(S1-PadMH4)")
  (net 7 "Net-(SW1-Pad2)")
  (net 8 "Net-(SW1-Pad3)")
  (net 9 "Net-(SW2-Pad3)")
  (net 10 "Net-(SW2-Pad2)")
  (net 11 "Net-(SW3-Pad3)")
  (net 12 "Net-(SW3-Pad2)")
  (net 13 "Net-(SW4-Pad3)")
  (net 14 "Net-(SW4-Pad2)")
  (net 15 "Net-(SW5-Pad3)")
  (net 16 "Net-(SW5-Pad2)")
  (net 17 "Net-(SW6-Pad3)")
  (net 18 "Net-(SW6-Pad2)")
  (net 19 "Net-(SW7-Pad3)")
  (net 20 "Net-(SW7-Pad2)")
  (net 21 "Net-(SW8-Pad3)")
  (net 22 "Net-(SW8-Pad2)")
  (net 23 "Net-(SW9-Pad3)")
  (net 24 "Net-(SW9-Pad2)")
  (net 25 "Net-(SW10-Pad3)")
  (net 26 "Net-(SW10-Pad2)")
  (net 27 "Net-(SW11-Pad3)")
  (net 28 "Net-(SW11-Pad2)")
  (net 29 "Net-(SW12-Pad3)")
  (net 30 "Net-(SW12-Pad2)")
  (net 31 "Net-(SW13-Pad3)")
  (net 32 "Net-(SW13-Pad2)")
  (net 33 "Net-(SW14-Pad3)")
  (net 34 "Net-(SW14-Pad2)")
  (net 35 "Net-(SW15-Pad3)")
  (net 36 "Net-(SW15-Pad2)")
  (net 37 "Net-(SW16-Pad3)")
  (net 38 "Net-(SW16-Pad2)")
  (net 39 "Net-(J1-Pad6)")
  (net 40 ICSP5)
  (net 41 ICSP4)
  (net 42 GND)
  (net 43 +5V)
  (net 44 "Net-(J1-Pad1)")
  (net 45 /+12VDC)
  (net 46 "Net-(J6-Pad2)")
  (net 47 "Net-(J6-Pad1)")
  (net 48 "Net-(R1-Pad2)")
  (net 49 "Net-(J6-Pad16)")
  (net 50 "Net-(J6-Pad15)")
  (net 51 "Net-(J6-Pad6)")
  (net 52 "Net-(J6-Pad5)")
  (net 53 "Net-(J6-Pad4)")
  (net 54 "Net-(J6-Pad3)")
  (net 55 "Net-(R2-Pad2)")
  (net 56 "Net-(R3-Pad2)")
  (net 57 "Net-(R4-Pad2)")
  (net 58 "Net-(R5-Pad2)")
  (net 59 "Net-(R6-Pad2)")
  (net 60 "Net-(R7-Pad2)")
  (net 61 "Net-(R8-Pad2)")
  (net 62 "Net-(R9-Pad2)")
  (net 63 "Net-(R10-Pad2)")
  (net 64 "Net-(R11-Pad2)")
  (net 65 "Net-(R12-Pad2)")
  (net 66 "Net-(R13-Pad2)")
  (net 67 "Net-(R14-Pad2)")
  (net 68 "Net-(R15-Pad2)")
  (net 69 "Net-(R16-Pad2)")
  (net 70 SW5L)
  (net 71 SW5)
  (net 72 SW8)
  (net 73 SW8L)
  (net 74 SW15L)
  (net 75 SW15)
  (net 76 SW4L)
  (net 77 SW4)
  (net 78 SW11L)
  (net 79 SW11)
  (net 80 SW16L)
  (net 81 SW16)
  (net 82 SW12L)
  (net 83 SW12)
  (net 84 SW7L)
  (net 85 SW7)
  (net 86 SW10L)
  (net 87 SW10)
  (net 88 SW3L)
  (net 89 SW3)
  (net 90 SW2L)
  (net 91 SW2)
  (net 92 SW14L)
  (net 93 SW14)
  (net 94 SW1L)
  (net 95 SW1)
  (net 96 SW9L)
  (net 97 SW9)
  (net 98 SW6L)
  (net 99 SW6)
  (net 100 SW13L)
  (net 101 SW13)
  (net 102 AN0)
  (net 103 AN1)
  (net 104 "Net-(D1-Pad1)")
  (net 105 "Net-(D2-Pad1)")
  (net 106 AN11)
  (net 107 CLK)
  (net 108 DAT)
  (net 109 STB)
  (net 110 "Net-(R19-Pad2)")
  (net 111 "Net-(D3-Pad2)")
  (net 112 "Net-(D3-Pad1)")
  (net 113 "Net-(D4-Pad2)")
  (net 114 "Net-(D4-Pad1)")
  (net 115 "Net-(D5-Pad2)")
  (net 116 "Net-(D5-Pad1)")
  (net 117 AN2)
  (net 118 AN3)
  (net 119 IN0)
  (net 120 IN1)
  (net 121 IN2)
  (net 122 JSW)
  (net 123 "Net-(D6-Pad1)")
  (net 124 "Net-(R23-Pad1)")
  (net 125 SCAN)
  (net 126 "Net-(U1-Pad5)")
  (net 127 "Net-(U2-Pad5)")
  (net 128 "Net-(U4-Pad5)")
  (net 129 "Net-(U5-Pad5)")
  (net 130 "Net-(J9-Pad1)")
  (net 131 "Net-(J3-Pad1)")
  (net 132 "Net-(J10-Pad2)")
  (net 133 "Net-(J11-Pad2)")
  (net 134 "Net-(J12-Pad2)")
  (net 135 "Net-(J13-Pad2)")
  (net 136 "Net-(D7-Pad2)")
  (net 137 "Net-(D7-Pad1)")
  (net 138 IN3)
  (net 139 "Net-(D8-Pad1)")
  (net 140 "Net-(D9-Pad1)")
  (net 141 "Net-(D10-Pad1)")
  (net 142 "Net-(R27-Pad1)")
  (net 143 "Net-(R28-Pad1)")
  (net 144 "Net-(R29-Pad1)")
  (net 145 "Net-(R18-Pad2)")
  (net 146 "Net-(U3-Pad18)")
  (net 147 "Net-(J2-Pad2)")
  (net 148 "Net-(D11-Pad2)")
  (net 149 "Net-(D11-Pad1)")
  (net 150 IN4)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /+12VDC)
    (add_net AN0)
    (add_net AN1)
    (add_net AN11)
    (add_net AN2)
    (add_net AN3)
    (add_net CLK)
    (add_net DAT)
    (add_net ICSP4)
    (add_net ICSP5)
    (add_net IN0)
    (add_net IN1)
    (add_net IN2)
    (add_net IN3)
    (add_net IN4)
    (add_net JSW)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J11-Pad2)")
    (add_net "Net-(J12-Pad2)")
    (add_net "Net-(J13-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad15)")
    (add_net "Net-(J6-Pad16)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(J6-Pad5)")
    (add_net "Net-(J6-Pad6)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R23-Pad1)")
    (add_net "Net-(R27-Pad1)")
    (add_net "Net-(R28-Pad1)")
    (add_net "Net-(R29-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(S1-PadB1)")
    (add_net "Net-(S1-PadD1)")
    (add_net "Net-(S1-PadMH1)")
    (add_net "Net-(S1-PadMH2)")
    (add_net "Net-(S1-PadMH3)")
    (add_net "Net-(S1-PadMH4)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(SW1-Pad3)")
    (add_net "Net-(SW10-Pad2)")
    (add_net "Net-(SW10-Pad3)")
    (add_net "Net-(SW11-Pad2)")
    (add_net "Net-(SW11-Pad3)")
    (add_net "Net-(SW12-Pad2)")
    (add_net "Net-(SW12-Pad3)")
    (add_net "Net-(SW13-Pad2)")
    (add_net "Net-(SW13-Pad3)")
    (add_net "Net-(SW14-Pad2)")
    (add_net "Net-(SW14-Pad3)")
    (add_net "Net-(SW15-Pad2)")
    (add_net "Net-(SW15-Pad3)")
    (add_net "Net-(SW16-Pad2)")
    (add_net "Net-(SW16-Pad3)")
    (add_net "Net-(SW2-Pad2)")
    (add_net "Net-(SW2-Pad3)")
    (add_net "Net-(SW3-Pad2)")
    (add_net "Net-(SW3-Pad3)")
    (add_net "Net-(SW4-Pad2)")
    (add_net "Net-(SW4-Pad3)")
    (add_net "Net-(SW5-Pad2)")
    (add_net "Net-(SW5-Pad3)")
    (add_net "Net-(SW6-Pad2)")
    (add_net "Net-(SW6-Pad3)")
    (add_net "Net-(SW7-Pad2)")
    (add_net "Net-(SW7-Pad3)")
    (add_net "Net-(SW8-Pad2)")
    (add_net "Net-(SW8-Pad3)")
    (add_net "Net-(SW9-Pad2)")
    (add_net "Net-(SW9-Pad3)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U3-Pad18)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U5-Pad5)")
    (add_net SCAN)
    (add_net STB)
    (add_net SW1)
    (add_net SW10)
    (add_net SW10L)
    (add_net SW11)
    (add_net SW11L)
    (add_net SW12)
    (add_net SW12L)
    (add_net SW13)
    (add_net SW13L)
    (add_net SW14)
    (add_net SW14L)
    (add_net SW15)
    (add_net SW15L)
    (add_net SW16)
    (add_net SW16L)
    (add_net SW1L)
    (add_net SW2)
    (add_net SW2L)
    (add_net SW3)
    (add_net SW3L)
    (add_net SW4)
    (add_net SW4L)
    (add_net SW5)
    (add_net SW5L)
    (add_net SW6)
    (add_net SW6L)
    (add_net SW7)
    (add_net SW7L)
    (add_net SW8)
    (add_net SW8L)
    (add_net SW9)
    (add_net SW9L)
  )
  (net_class GND ""
    (clearance 0.3)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module control-surface:THB001P (layer F.Cu) (tedit 60DA8E16)
    (at 171.958 119.126 270)
    (descr THB001P-5)
    (tags Switch)
    (fp_text reference S1 (at -2.286 6.858 90) (layer F.SilkS))
    (fp_text value THB001P (at -1.778 11.43 90) (layer F.SilkS) hide)
    (fp_text user %R (at -2.286 6.858 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.4826 -0.6604 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 2 thru_hole circle (at -3.048 -0.6604 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 102 AN0))
    (pad 3 thru_hole circle (at -5.588 -0.6604 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 11 thru_hole circle (at 6.985 11.43 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 12 thru_hole circle (at 6.985 8.89 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 103 AN1))
    (pad 13 thru_hole circle (at 6.985 6.35 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad A1 thru_hole circle (at -6.35 17.526 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad B1 thru_hole circle (at 0.254 17.526 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(S1-PadB1)"))
    (pad C1 thru_hole circle (at -6.35 22.098 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 122 JSW))
    (pad D1 thru_hole circle (at 0.254 22.098 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(S1-PadD1)"))
    (pad MH1 thru_hole circle (at 4.826 2.54 270) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(S1-PadMH1)"))
    (pad MH2 thru_hole circle (at -10.795 2.54 270) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 "Net-(S1-PadMH2)"))
    (pad MH3 thru_hole circle (at -10.795 15.875 270) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 "Net-(S1-PadMH3)"))
    (pad MH4 thru_hole circle (at 4.826 15.875 270) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 "Net-(S1-PadMH4)"))
    (model C:/RPL/banbury/VS1053/ALPS-JOYSTICK.STEP
      (offset (xyz -11.25 -35.5 22))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -180))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 161.7 76 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R34 (at 2.54 -1.92) (layer F.SilkS))
    (fp_text value R_Small_US (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 149 "Net-(D11-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 150 IN4))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_T-1_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 156.6 73)
    (descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (fp_text reference D11 (at 2.54 -2.42) (layer F.SilkS))
    (fp_text value 1N4004 (at 2.54 2.42) (layer F.Fab))
    (fp_text user K (at 0 -2) (layer F.SilkS))
    (fp_text user K (at 0 -2) (layer F.Fab))
    (fp_text user %R (at 2.78 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 148 "Net-(D11-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 149 "Net-(D11-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module control-surface:thonkiconn_fuzzySi (layer F.Cu) (tedit 560B1645)
    (at 159.8 64.3 180)
    (fp_text reference J2 (at 3.81 6.35) (layer F.SilkS))
    (fp_text value fuzzySI_thonkiconn (at 0 -7.62) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 6.48 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 42 GND))
    (pad 2 thru_hole rect (at 0 3.38 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 147 "Net-(J2-Pad2)"))
    (pad 3 thru_hole rect (at 0 -4.92 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 148 "Net-(D11-Pad2)"))
    (model /home/mary/Dropbox/working/Templates/thonkiconn_fuzzySi_3d_v6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 -90))
    )
    (model ${KIPRJMOD}/WQP-PJ398SM.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm_Clear (layer F.Cu) (tedit 5A6C9BC0)
    (at 197.5 57.25)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (fp_text reference D10 (at -3.06244 -1.47314) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (fp_text user %R (at 1.47 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 141 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 203.7 123.3 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R33 (at -2.6 0 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 120 IN1))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 42 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 189.55 122.8 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R32 (at -3.1 -0.05 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 121 IN2))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 42 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 177.75 125.5 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R31 (at 2.54 -1.92) (layer F.SilkS))
    (fp_text value R_Small_US (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 138 IN3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 125.9 124.4)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R30 (at -1.7 0 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 119 IN0))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 42 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 199.75 65.75 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R29 (at 7.53056 0.00212 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 141 "Net-(D10-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 144 "Net-(R29-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 188.25 65.75 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R28 (at 7.51572 -0.00724 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 143 "Net-(R28-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 140 "Net-(D9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 176.75 65.75 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R27 (at 3.81 -1.92 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 139 "Net-(D8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 142 "Net-(R27-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 205.90256 119.31396)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R26 (at 7.69744 -0.06396) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 137 "Net-(D7-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 138 IN3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 156.3 79.1)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R24 (at 3.81 -1.92) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 211.5 65.75 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R23 (at -1.75 0.55) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 123 "Net-(D6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 124 "Net-(R23-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 203.9 85.6)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R22 (at -3.05 -0.8) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 116 "Net-(D5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 121 IN2))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 206.38262 113.29924)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R21 (at 7.56738 0.10076) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 114 "Net-(D4-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 120 IN1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 205.7654 125.8316)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R20 (at 2.4846 2.1684) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 112 "Net-(D3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 119 IN0))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 130.95 126.9 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R18 (at 6.7 -0.4 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 145 "Net-(R18-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 104 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 108.1532 94.4372 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R17 (at 3.81 -1.92 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 44 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 146.05 71.12)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R16 (at 3.81 -1.92) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 69 "Net-(R16-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 74 SW15L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 166.09314 71.55434)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R15 (at 7.55686 0.09566) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 68 "Net-(R15-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 80 SW16L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 191.77 82.55)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R14 (at 7.78 0.55) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 67 "Net-(R14-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 92 SW14L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 202.692 108.585 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R13 (at -2.735 0.092 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 66 "Net-(R13-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 100 SW13L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 161.29 82.55)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R12 (at 1.66 -2.1) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 65 "Net-(R12-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 82 SW12L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 151.13 82.55)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R11 (at 4.92 -2) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 64 "Net-(R11-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 78 SW11L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 171.45 82.55)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R10 (at 7.55 0.05) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 63 "Net-(R10-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 86 SW10L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 176.53 107.823 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R9 (at 3.81 -1.92 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 62 "Net-(R9-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 96 SW9L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 135.89 71.12)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R8 (at 3.81 -1.92) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 61 "Net-(R8-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 73 SW8L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 176.26076 71.5264)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R7 (at 7.28924 0.1736) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 60 "Net-(R7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 84 SW7L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 201.3 118.15 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at 7.2939 -0.01158 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 59 "Net-(R6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 98 SW6L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 130.9624 82.5754)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 7.1876 0.0246) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 58 "Net-(R5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 70 SW5L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 140.97 82.55)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 7.23 0.05) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 57 "Net-(R4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 76 SW4L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 181.61 82.55)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 7.09 0.1) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 56 "Net-(R3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 90 SW2L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 176.53 118.11 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 3.81 -1.92 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 55 "Net-(R2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 94 SW1L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 186.62904 71.55688)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 7.22096 0.09312) (layer F.SilkS))
    (fp_text value R_Small_US (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 48 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 88 SW3L))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 128.5 110.3)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R25 (at -2.7724 -0.4052) (layer F.SilkS))
    (fp_text value 220 (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 131 "Net-(J3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 43 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 140.97 111.76 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R19 (at 3.1242 2.286) (layer F.SilkS))
    (fp_text value 220 (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 110 "Net-(R19-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 130 "Net-(J9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm_Clear (layer F.Cu) (tedit 5A6C9BC0)
    (at 185.75 57.25)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (fp_text reference D9 (at -2.32848 -1.41272 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (fp_text user %R (at 1.47 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 140 "Net-(D9-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 +5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm_Clear (layer F.Cu) (tedit 5A6C9BC0)
    (at 174.5 57.25)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (fp_text reference D8 (at -2.51912 -1.39322) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (fp_text user %R (at 1.47 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 139 "Net-(D8-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 +5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_T-1_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 213.12124 116.29898 180)
    (descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (fp_text reference D7 (at 7.53872 0.0127) (layer F.SilkS))
    (fp_text value 1N4004 (at 2.54 2.42) (layer F.Fab))
    (fp_text user K (at -1.72876 0.09898) (layer F.SilkS))
    (fp_text user K (at 0 -2) (layer F.Fab))
    (fp_text user %R (at 2.78 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 136 "Net-(D7-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 137 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module control-surface:thonkiconn_fuzzySi (layer F.Cu) (tedit 560B1645)
    (at 170.942 64.262 180)
    (fp_text reference J13 (at 3.81 6.35 270) (layer F.SilkS))
    (fp_text value fuzzySI_thonkiconn (at 0 -7.62) (layer F.Fab) hide)
    (pad 3 thru_hole rect (at 0 -4.92 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 136 "Net-(D7-Pad2)"))
    (pad 2 thru_hole rect (at 0 3.38 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 135 "Net-(J13-Pad2)"))
    (pad 1 thru_hole rect (at 0 6.48 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 42 GND))
    (model ${KIPRJMOD}/WQP-PJ398SM.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module control-surface:thonkiconn_fuzzySi (layer F.Cu) (tedit 560B1645)
    (at 194 64.25 180)
    (fp_text reference J12 (at 3.65146 6.5223 270) (layer F.SilkS))
    (fp_text value fuzzySI_thonkiconn (at 0 -7.62) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 6.48 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 42 GND))
    (pad 2 thru_hole rect (at 0 3.38 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 134 "Net-(J12-Pad2)"))
    (pad 3 thru_hole rect (at 0 -4.92 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(D4-Pad2)"))
    (model ${KIPRJMOD}/WQP-PJ398SM.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module control-surface:thonkiconn_fuzzySi (layer F.Cu) (tedit 560B1645)
    (at 182.5 64.25 180)
    (fp_text reference J11 (at 2.922 6.338 270) (layer F.SilkS))
    (fp_text value fuzzySI_thonkiconn (at 0 -7.62) (layer F.Fab) hide)
    (pad 3 thru_hole rect (at 0 -4.92 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(D3-Pad2)"))
    (pad 2 thru_hole rect (at 0 3.38 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 133 "Net-(J11-Pad2)"))
    (pad 1 thru_hole rect (at 0 6.48 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 42 GND))
    (model ${KIPRJMOD}/WQP-PJ398SM.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module control-surface:thonkiconn_fuzzySi (layer F.Cu) (tedit 560B1645)
    (at 205.5 64.25 180)
    (fp_text reference J10 (at 2.808 6.338 270) (layer F.SilkS))
    (fp_text value fuzzySI_thonkiconn (at 0 -7.62) (layer F.Fab) hide)
    (pad 3 thru_hole rect (at 0 -4.92 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(D5-Pad2)"))
    (pad 2 thru_hole rect (at 0 3.38 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 132 "Net-(J10-Pad2)"))
    (pad 1 thru_hole rect (at 0 6.48 180) (size 2.5 1) (drill oval 1.5 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 42 GND))
    (model ${KIPRJMOD}/WQP-PJ398SM.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 132.08 85.09)
    (fp_text reference SW5 (at 2.54 2.54) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 58 "Net-(R5-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(SW5-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(SW5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 71 SW5))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork (layer F.Cu) (tedit 5A1DC084)
    (at 144.1 113)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (fp_text reference J9 (at 0.5 2.3) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 -1.8) (layer F.Fab))
    (fp_text user %R (at 0 1.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 130 "Net-(J9-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork (layer F.Cu) (tedit 5A1DC084)
    (at 144.1 110.6)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (fp_text reference J3 (at 0 1.8) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 -1.8) (layer F.Fab))
    (fp_text user %R (at 0 1.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 131 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 132.461 78.4225 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C7 (at 6.93674 0.35306 180) (layer F.SilkS))
    (fp_text value C_Small (at 2.5 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 198.23176 72.4662 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 7.3279 -0.15748 180) (layer F.SilkS))
    (fp_text value C_Small (at 2.5 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 154.0256 95.7326 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C5 (at 7.81558 -0.13208) (layer F.SilkS))
    (fp_text value C_Small (at 2.5 2.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 193.04 85.09)
    (fp_text reference SW14 (at 1.49352 8.57504) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 67 "Net-(R14-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(SW14-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(SW14-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 93 SW14))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm_LongPads (layer F.Cu) (tedit 5A02E8C5)
    (at 181.2798 103.6574 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U5 (at -2.5273 -1.01092 180) (layer F.SilkS))
    (fp_text value UCN5821 (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 SW2L))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 SW2))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 SW14L))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 STB))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 SW14))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 129 "Net-(U5-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 SW6))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 SW13))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 SW6L))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 "Net-(U4-Pad5)"))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 100 SW13L))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 CLK))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm_LongPads (layer F.Cu) (tedit 5A02E8C5)
    (at 158.5468 104.1654 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U4 (at 0.35306 -2.37998 270) (layer F.SilkS))
    (fp_text value UCN5821 (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 SW10L))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 SW10))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 SW3L))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 STB))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 SW3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 "Net-(U4-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 SW9L))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 SW1L))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 SW9))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 "Net-(U2-Pad5)"))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 SW1))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 CLK))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 162.56 85.09)
    (fp_text reference SW12 (at 2.032 8.382) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 65 "Net-(R12-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(SW12-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(SW12-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 83 SW12))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm_LongPads (layer F.Cu) (tedit 5A02E8C5)
    (at 135.636 106.807 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U2 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value UCN5821 (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 SW11L))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 SW11))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 SW16L))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 STB))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 SW16))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 "Net-(U2-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 SW12L))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 SW12))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 SW7L))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "Net-(U1-Pad5)"))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 SW7))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 CLK))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical (layer F.Cu) (tedit 5C6C6C14)
    (at 110.9472 86.6902)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (fp_text reference RV1 (at 10.80516 9.83234 180) (layer F.SilkS))
    (fp_text value R_POT (at 0 9.86 180) (layer F.Fab))
    (fp_text user %R (at 7.62 2.54) (layer F.Fab))
    (pad "" thru_hole oval (at 7.5 -2.3 90) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 90) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 2 thru_hole circle (at 0 2.5 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 106 AN11))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 43 +5V))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/ALPHA-RD901F-40.step
      (offset (xyz 7.5 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm_LongPads (layer F.Cu) (tedit 5A02E8C5)
    (at 112.522 106.807 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U1 (at 0.381 -3.048 180) (layer F.SilkS))
    (fp_text value UCN5821 (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 SW8L))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 SW8))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 SW5L))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 STB))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 SW5))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "Net-(U1-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 SW15L))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 SW15))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 SW4L))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 DAT))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 SW4))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 CLK))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm_Clear (layer F.Cu) (tedit 5A6C9BC0)
    (at 209 57.25)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (fp_text reference D6 (at -2.96832 -1.60026) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (fp_text user %R (at 1.47 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 123 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical (layer F.Cu) (tedit 5C6C6C14)
    (at 202.5 95.1)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (fp_text reference RV3 (at -0.99568 -4.89966 180) (layer F.SilkS))
    (fp_text value R_POT (at 0 9.86 180) (layer F.Fab))
    (fp_text user %R (at 7.62 2.54) (layer F.Fab))
    (pad "" thru_hole oval (at 7.5 -2.3 90) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 90) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 2 thru_hole circle (at 0 2.5 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 118 AN3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 43 +5V))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl
      (offset (xyz -2 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/ALPHA-RD901F-40.step
      (offset (xyz 7.5 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical (layer F.Cu) (tedit 5C6C6C14)
    (at 202.565 74.3966)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (fp_text reference RV2 (at -2.915 6.9534 180) (layer F.SilkS))
    (fp_text value R_POT (at 0 9.86 180) (layer F.Fab))
    (fp_text user %R (at 7.62 2.54) (layer F.Fab))
    (pad "" thru_hole oval (at 7.5 -2.3 90) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 90) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 2 thru_hole circle (at 0 2.5 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 117 AN2))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 43 +5V))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/ALPHA-RD901F-40.step
      (offset (xyz 7.5 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Diode_THT:D_T-1_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 212.79612 106.49458 180)
    (descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (fp_text reference D5 (at 7.5692 -0.12446) (layer F.SilkS))
    (fp_text value 1N4004 (at 2.54 2.42) (layer F.Fab))
    (fp_text user K (at 0 -2) (layer F.SilkS) hide)
    (fp_text user K (at 0 -2) (layer F.Fab))
    (fp_text user %R (at 2.78 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 115 "Net-(D5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 116 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_T-1_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 212.81898 110.236 180)
    (descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (fp_text reference D4 (at 7.44982 0.13462) (layer F.SilkS))
    (fp_text value 1N4004 (at 2.54 2.42) (layer F.Fab))
    (fp_text user K (at -2.413 2.667) (layer F.SilkS) hide)
    (fp_text user K (at 0 -2) (layer F.Fab) hide)
    (fp_text user %R (at 2.78 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 113 "Net-(D4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 114 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_T-1_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 211.709 122.428 180)
    (descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (fp_text reference D3 (at -2.391 0.028) (layer F.SilkS))
    (fp_text value 1N4004 (at 2.54 2.42) (layer F.Fab))
    (fp_text user K (at -1.941 -2.422) (layer F.SilkS) hide)
    (fp_text user K (at 0 -2) (layer F.Fab))
    (fp_text user %R (at 2.78 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 111 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 109.0676 99.06 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 2.6162 2.4638 270) (layer F.SilkS))
    (fp_text value C_Small (at 2.5 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 133.731 94.615 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C3 (at -2.667 0) (layer F.SilkS))
    (fp_text value C_Small (at 2.5 2.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 107.3658 81.5086 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 7.366 -0.381 180) (layer F.SilkS))
    (fp_text value C_Small (at 2.5 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 124.0536 62.27064 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 10.77976 0.12446) (layer F.SilkS))
    (fp_text value 1N4004 (at 5.08 2.47) (layer F.Fab))
    (fp_text user K (at 0 -2.1) (layer F.Fab))
    (fp_text user K (at 0 -2.1) (layer F.Fab))
    (fp_text user %R (at 5.47 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 /+12VDC))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 105 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 144.526 123.698 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 0.254 3.2258 180) (layer F.SilkS))
    (fp_text value C_Small (at 2.5 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm_Clear (layer F.Cu) (tedit 5A6C9BC0)
    (at 133.4389 125.6538)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (fp_text reference D1 (at 5.0111 1.9962) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (fp_text user %R (at 1.47 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 104 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 147.32 73.66)
    (fp_text reference SW15 (at 9.144 4.572) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 69 "Net-(R16-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(SW15-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(SW15-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 75 SW15))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 137.16 73.66)
    (fp_text reference SW8 (at 2.286106 1.981309) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 61 "Net-(R8-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 "Net-(SW8-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 "Net-(SW8-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 72 SW8))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 142.24 85.09)
    (fp_text reference SW4 (at 2.032 8.636) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 57 "Net-(R4-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(SW4-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(SW4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 77 SW4))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown (layer F.Cu) (tedit 5AC8BA0D)
    (at 110.1852 73.8378 270)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (fp_text reference U6 (at -3.80746 -20.01012 180) (layer F.SilkS))
    (fp_text value LM7805_TO220 (at 2.54 2 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -20.58 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 105 "Net-(D2-Pad1)"))
    (pad "" np_thru_hole oval (at 2.54 -16.66 270) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 108.966 68.58 90)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference J6 (at -3.06324 -1.9812 180) (layer F.SilkS))
    (fp_text value Conn_02x08_Odd_Even (at 1.27 20.11 90) (layer F.Fab))
    (fp_text user %R (at 1.27 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J6-Pad16)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J6-Pad15)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /+12VDC))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /+12VDC))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J6-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(J6-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(J6-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(J6-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl
      (offset (xyz 2.5 0 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 0))
    )
  )
  (module Package_DIP:DIP-28_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 107.95 121.92 90)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at 10.0838 -0.9906 90) (layer F.SilkS))
    (fp_text value PIC18F25K20_ISS (at 3.81 35.35 90) (layer F.Fab))
    (fp_text user %R (at 3.81 16.51 90) (layer F.Fab))
    (pad 28 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 ICSP4))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 CLK))
    (pad 27 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 ICSP5))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 IN2))
    (pad 26 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 124 "Net-(R23-Pad1)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 IN1))
    (pad 25 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 106 AN11))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 IN0))
    (pad 24 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 STB))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 145 "Net-(R18-Pad2)"))
    (pad 23 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 142 "Net-(R27-Pad1)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 150 IN4))
    (pad 22 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 143 "Net-(R28-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 21 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 138 IN3))
    (pad 20 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 JSW))
    (pad 19 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 AN3))
    (pad 18 thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 146 "Net-(U3-Pad18)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 AN2))
    (pad 17 thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(R19-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 AN1))
    (pad 16 thru_hole oval (at 7.62 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 DAT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 AN0))
    (pad 15 thru_hole oval (at 7.62 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 144 "Net-(R29-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 107.8992 126.0094 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J1 (at 2.54 0.254 180) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 ICSP5))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 ICSP4))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (offset (xyz 0 0 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 0))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 193.04 109.22)
    (fp_text reference SW13 (at -1.64 -1.82) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 101 SW13))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(SW13-Pad2)"))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(SW13-Pad3)"))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 "Net-(R13-Pad2)"))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 181.61 109.22)
    (fp_text reference SW9 (at 2.15138 -2.37998) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 62 "Net-(R9-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(SW9-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "Net-(SW9-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 97 SW9))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 193.04 118.11)
    (fp_text reference SW6 (at 2.032 8.636) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 59 "Net-(R6-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(SW6-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "Net-(SW6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 99 SW6))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 187.96 73.66)
    (fp_text reference SW3 (at 7.874 2.794 90) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 48 "Net-(R1-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(SW3-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(SW3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 89 SW3))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 167.64 73.66)
    (fp_text reference SW16 (at -4.572 4.318) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 68 "Net-(R15-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "Net-(SW16-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(SW16-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 81 SW16))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 172.72 85.09)
    (fp_text reference SW10 (at 2.54 8.382) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 63 "Net-(R10-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(SW10-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 "Net-(SW10-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 87 SW10))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 152.4 85.09)
    (fp_text reference SW11 (at 2.54508 8.41502) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 64 "Net-(R11-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(SW11-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(SW11-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 79 SW11))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 177.8 73.66)
    (fp_text reference SW7 (at 2.286 2.413) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 60 "Net-(R7-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "Net-(SW7-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(SW7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 85 SW7))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 182.88 85.09)
    (fp_text reference SW2 (at 2.54 8.636) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 56 "Net-(R3-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(SW2-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(SW2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 91 SW2))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module control-surface:ILSTA (layer F.Cu) (tedit 5FFE314B)
    (at 181.61 118.11)
    (fp_text reference SW1 (at 1.778 8.89) (layer F.SilkS))
    (fp_text value ILSTA180 (at 0 -0.5) (layer F.Fab))
    (pad 6 thru_hole circle (at 5.1562 3.2512) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 55 "Net-(R2-Pad2)"))
    (pad 5 thru_hole circle (at -0.6604 3.2766) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5V))
    (pad 4 thru_hole circle (at 4.5 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 SCAN))
    (pad 3 thru_hole circle (at 0 6.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(SW1-Pad3)"))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(SW1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 95 SW1))
    (model ":downloads:CKCOMPONENTS_ILSTA18030(3)/ILS TA180 30.stp"
      (offset (xyz 2.2 -3.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (gr_line (start 150.75 68.05) (end 151.1 67.58) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.42392 67.6) (end 130.9 68.05) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.1 67.58) (end 151.1 54.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.9 68.05) (end 150.75 68.05) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.43408 58.39206) (end 130.42392 67.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.3592 58.42) (end 130.43408 58.39206) (layer Edge.Cuts) (width 0.1))
  (gr_text "control surface rev 2" (at 148.0312 127.0508) (layer F.SilkS))
  (gr_text J5 (at 146.812 115.062) (layer B.SilkS))
  (gr_text J9 (at 146.812 112.522) (layer B.SilkS))
  (gr_text "MIDI\nOUT" (at 146.5 109.9) (layer B.SilkS))
  (gr_text "CONTROL\nSURFACE\nrev 2" (at 163.322 115.316) (layer B.SilkS))
  (gr_text ICSP (at 116.10848 128.21666) (layer B.SilkS))
  (gr_text "-12 red line" (at 124.67082 59.57062) (layer B.SilkS))
  (gr_text J1 (at 108.08208 123.46178) (layer B.SilkS))
  (gr_line (start 215.2904 54.5) (end 151.1 54.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 215.2904 129.032) (end 215.2904 54.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.3592 129.032) (end 215.2904 129.032) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.3592 58.42) (end 105.3592 129.032) (layer Edge.Cuts) (width 0.1))
  (zone (net 42) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.172 63.881) (xy 105.918 128.397) (xy 214.0204 128.4478) (xy 214.4088 54.6165) (xy 152.3312 54.7435)
        (xy 150.0886 59.69) (xy 107.7722 59.4868)
      )
    )
  )
)
