(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 152)
    (tracks 17)
    (zones 0)
    (modules 5)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6.1 3.5)
    (pad_drill 6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7EFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 623500D2)
    (at 73.861 125.4524)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 7.564 4.32768) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 6.1 3.5) (drill oval 6 3.4) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 623500D2)
    (at 7.45 125.18008)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at -6.665 4.85268) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 6.1 3.5) (drill oval 6 3.4) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 623500D2)
    (at 73.861 3.053)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 6.1 3.5) (drill oval 6 3.4) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 623500D2)
    (at 7.45 3.00508)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 6.1 3.5) (drill oval 6 3.4) (layers *.Cu *.Mask))
  )
  (module lappi-plate-r1:rantbot-logo-1 (layer F.Cu) (tedit 5F933F22)
    (at 41.625 124.08008)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text "DELTA V" (at 15.1 58.20508) (layer F.Cu))
  (gr_text "CTRL\nSURF" (at 68.375 15.05) (layer F.Cu))
  (gr_text Chord (at 52.975 98.08008) (layer F.Cu))
  (gr_text Arp (at 29.925 97.98008) (layer F.Cu))
  (gr_text "MODE\nLOCK" (at 74 81.65508) (layer F.Cu))
  (gr_text ACCENT (at 15.4 46.40508) (layer F.Cu))
  (gr_text VOICE (at 48.15 24.85508) (layer F.Cu))
  (gr_text BANK (at 27.55 24.95508) (layer F.Cu))
  (gr_text ADVANCE (at 15.7 34.70508) (layer F.Cu))
  (gr_text CHORD (at 14.3 23.50508) (layer F.Cu))
  (gr_text ARP (at 12.7 11.90508) (layer F.Cu))
  (gr_text PRESET (at 68 33.80508) (layer F.Cu))
  (gr_text "MIDI\nOUT" (at 15.1 91.80508) (layer F.Cu))
  (gr_line (start 0.25 128.50758) (end 0.25 0.00508) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.25 0.00508) (end 81 0.00758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 81 0.00758) (end 81 128.50508) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 81 128.50508) (end 0.25 128.50758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 24.62738 87.50758) (end 24.62738 80.80758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 24.62738 80.80758) (end 30.84738 80.80758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.84738 80.80758) (end 30.84738 87.50758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.84738 87.50758) (end 24.62738 87.50758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 24.62738 77.30758) (end 24.62738 70.60758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 24.62738 70.60758) (end 30.84738 70.60758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.84738 70.60758) (end 30.84738 77.30758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.84738 77.30758) (end 24.62738 77.30758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 24.62738 57.00758) (end 24.62738 50.30758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 24.62738 50.30758) (end 30.84738 50.30758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.84738 50.30758) (end 30.84738 57.00758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.84738 57.00758) (end 24.62738 57.00758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 24.62738 46.85758) (end 24.62738 40.15758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 24.62738 40.15758) (end 30.84738 40.15758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.84738 40.15758) (end 30.84738 46.85758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.84738 46.85758) (end 24.62738 46.85758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 24.62738 36.70758) (end 24.62738 30.00758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 24.62738 30.00758) (end 30.84738 30.00758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.84738 30.00758) (end 30.84738 36.70758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.84738 36.70758) (end 24.62738 36.70758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.12738 92.60758) (end 36.12738 85.90758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.12738 85.90758) (end 42.34738 85.90758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.34738 85.90758) (end 42.34738 92.60758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.34738 92.60758) (end 36.12738 92.60758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.12738 82.40758) (end 36.12738 75.70758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.12738 75.70758) (end 42.34738 75.70758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.34738 75.70758) (end 42.34738 82.40758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.34738 82.40758) (end 36.12738 82.40758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.12738 72.20758) (end 36.12738 65.50758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.12738 65.50758) (end 42.34738 65.50758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.34738 65.50758) (end 42.34738 72.20758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.34738 72.20758) (end 36.12738 72.20758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.12738 62.05758) (end 36.12738 55.35758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.12738 55.35758) (end 42.34738 55.35758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.34738 55.35758) (end 42.34738 62.05758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.34738 62.05758) (end 36.12738 62.05758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.12738 51.90758) (end 36.12738 45.20758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.12738 45.20758) (end 42.34738 45.20758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.34738 45.20758) (end 42.34738 51.90758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.34738 51.90758) (end 36.12738 51.90758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.12738 41.75758) (end 36.12738 35.05758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.12738 35.05758) (end 42.34738 35.05758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.34738 35.05758) (end 42.34738 41.75758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.34738 41.75758) (end 36.12738 41.75758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.12738 31.60758) (end 36.12738 24.90758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.12738 24.90758) (end 42.34738 24.90758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.34738 24.90758) (end 42.34738 31.60758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.34738 31.60758) (end 36.12738 31.60758) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.31738 42.59058) (end 60.31738 36.21258) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.31738 36.21258) (end 66.43738 36.21258) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 66.43738 36.21258) (end 66.43738 42.59058) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 66.43738 42.59058) (end 60.31738 42.59058) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.23138 31.12658) (end 60.23138 24.83458) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.23138 24.83458) (end 66.43738 24.83458) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 66.43738 24.83458) (end 66.43738 31.12658) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 66.43738 31.12658) (end 60.23138 31.12658) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.10938 42.67658) (end 69.10938 36.38458) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.10938 36.38458) (end 75.22938 36.38458) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.22938 36.38458) (end 75.22938 42.67658) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.22938 42.67658) (end 69.10938 42.67658) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.36838 31.12658) (end 69.36838 24.83458) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.36838 24.83458) (end 75.22938 24.83458) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.22938 24.83458) (end 75.22938 31.12658) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.22938 31.12658) (end 69.36838 31.12658) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7.35 102.75508) (xy 7.35 87.55508) (xy 15.1 84.45508) (xy 22.95 87.55508) (xy 22.95 102.80508)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.75 75.95508) (xy 73.45 93.95508) (xy 78.9 94.45508) (xy 80.05 92.90508) (xy 80.05 84.15508)
        (xy 80.05 65.65508)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 10))
    (polygon
      (pts
        (xy 22.9 3.45508) (xy 22.824999 29.68008) (xy 32.425001 29.68008) (xy 32.5 3.35508)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 10))
    (polygon
      (pts
        (xy 43.35 3.394926) (xy 43.275003 29.60508) (xy 52.874997 29.60508) (xy 52.95 3.294926)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 2))
    (polygon
      (pts
        (xy 29.2 94.85508) (xy 28.918774 115.768768) (xy 54.931226 115.931232) (xy 55.212489 94.967617)
      )
    )
  )
)
